

**No:** 814/19/2

**Place and date : Podgorica, 15.02.2019.**

„13 Jul Plantaže” A.D., Podgorica announces on the website :

**AMENDMENTS**

**TO THE REQUEST FOR COLECTING THE BIDS**

**FOR THE PROCEDURE OF PROCUREMENT**

**of the Spring pruning machine , Herbicide sprayer, Sucker remover**

1. Amendment to the Request for Collecting the Bids for Procedure of Procurement of the Goods –Spring pruning machine, herbicide sprayer, sucker remover, shall be made on the pages No.8/43 and 9/43, in the section TECHNICAL CHARACTERISTICS OR SPECIFICATIONS OF THE PROCUREMENT SUBJECT , NAMELY BILL OF QUANTITIES for the Lot No.1 in the following manner:

Deleted:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Ord.No.** | **Description of the subject of the procurement, ie a part of the subject of procurement** | **Important characteristics of the subject of the procurement concerning quality, performances and/or measures** | **Unit of measure** | **Quantity** |
| 1 | Spring pruning machine | Max. height of the posts 2,5 m  Cloth 40 cm  Working height above the ground  from 40 to 70 cm  Frame for the support with vertical hydraulic movement (80 cm) and horizontal hydraulic movement (60 cm)  Telescopic frame for adaptation of the height of the bridge of the posts  Mechanically adapted width of the head (from 74 to 80 cm)  Insulation of the upper part with the system of small brushes in two layers, separated by PVC cloth  Upper bearers of the small brushes , made of stainless steel that may be opened by the compass for the internal control  Frame with safety device in case of the impact  Guides with elastic return for posts  Elastic post for nozzles  Kit for the possibility of using the machine for eliminating grass  Mixed system for dispersing in spray or contact  Two lots of nozzles for covering in the working conditions  Pipes, 5 metres longs for connecting the machine  Hydraulic pipes with fast joints for the attachment to the distributor of the tractor  Attachment to the tractor T4 95F New Holland | pieces | 6 |

And replaced by:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Ord.No.** | **Description of the subject of the procurement, ie a part of the subject of procurement** | **Important characteristics of the subject of the procurement concerning quality, performances and/or measures** | **Unit of measure** | **Quantity** |
| 1 | Spring pruning machine | Max. height of the posts 2,5 m  Working height above the ground  from 40 to 70 cm  Vertical cutting device 1,65-1,95 m  Horizontal cutting device on both sides 0,80 m  Necessary hydraulic flow 20-30 l/m  Height of movement 500x2 mm  Lateral movement 500x2 mm  Transverse slope +35 □ / -15 □  Number of hydraulic movements up to 8  Electrohydraulic controls  Conveyor  Attachment to the tractor T4 95F New Holland  Single tied knives of the vertical and horizontal cutting device  Electro-hydraulic commands with two flow regulators and inlet filter , with joystick , plate for hanging at 3 points | pieces | 6 |

Procurer announces the amendments to the concerned Request on the website: www.plantaze.com.

Committee for opening and evaluation of the bids,

Presiding,

Goran Milić, grad.lawyer