**No. : 5084/3**

**Podgorica, 13.09.2023**

**MODIFICATIONS AND AMENDMENTS**

**Request for Collecting the Bids for Procurement of the Barriques No. 5084/1 dated from 04.09.2023, for the procedure of procurement of the goods – barriques**

In the text of the Request, Procurer changes in the page 8 out of 18 of the Request- item 1-barriques for red wines - **in the section Technical characteristics /specification:Barriques-quantities,** in the manner, as it follows:

**Instead of the text**:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Ord.**  **No.** | **Description of the subject of the procurement, ie of the part of the subject of procurement** | **Essential characteristics of the subject of procurement concerning quality, performances and/or measures** | **Unit of measure** | **Quantity** |
| **1.** | Barriques  for red wines | Barrique volume 225 lit  French oak, Sessilee oak  Middle oak granules, 3-5 mm  Height: 935 mm (+/- 5mm)  For aging 10-12 months  Diameter of the 'head' ( top cover of the barrique): 575 mm(+/-2,5mm)  Diameter of barrique: 690mm (+/- 2,5 mm)  Thickness of the staves, the barrique is made of: 27 mm  Upper hole on the barrique diameter 50mm  Upper hole should be conical and toasted MT+  Bung for hole, normal and silicon  Grain type: middle to narrow  Toasting of the barrique staves: medium +toasting  No. of the zinc coated hoops: 6  -Thallus: 55x2 (+/-1 %)-H: 55mm (+/- 1mm)  -Circle of barrique: 35x2 (+/-1%)- H: 110 mm (+/- 5mm)  -Diameter: 45x2 (+/- 1%) –H: 320 mm(+/- 5mm)  necessary toasting of the barrique covers  intensity of cover toasting: medium + toasting | pcs | 94 |

**The following text should be written :**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Ord.**  **No.** | **Description of the subject of the procurement, ie of the part of the subject of procurement** | **Essential characteristics of the subject of procurement concerning quality, performances and/or measures** | **Unit of measure** | **Quantity** |
| **1.** | Barriques  for red wines | Barrique volume 225 lit  French oak, Sessilee oak  Middle oak granules, 3-5 mm  Height: 935 mm (+/- 5mm)  For aging 10-12 months  Diameter of the 'head' ( top cover of the barrique): 575 mm(+/-2,5mm)  Diameter of barrique: 690mm (+/- 2,5 mm)  Thickness of the staves, the barrique is made of: 27 mm  Upper hole on the barrique diameter 50mm  Upper hole should be conical and toasted MT+  Bung for hole, normal and silicon  Grain type: middle to narrow  Toasting of the barrique staves: medium +toasting  No. of the zinc coated hoops: 6  -Thallus: 55x2 (+/-1 %)-H: 55mm (+/- 1mm)  -Circle of barrique: 35x2 (+/-1%)- H: 110 mm (+/- 5mm)  -Diameter: 45x2 (+/- 1%) –H: 320 mm(+/- 5mm)  necessary toasting of the barrique covers  intensity of cover toasting: medium + toasting | pcs | 113 |

**Chairman of the Committee**

**for opening and evaluation of the bids**

**Bojan Gašović**