**SUBJECT: REQUEST FOR THE COLLECTION OF OFFERS FOR CLOSURES AND PVC CAPS**

**CORK STOPPERS**

* Closures for premium white and red wines for the bottle, volume 0,75 lit with inner diameter of the neck 17,5-18,5 mm for keeping up to 3 years. The orientational quantity is 4.500.000 pcs. The length of the closure must be offered in the size up to 44 mm.
* Closures for premium white and red wines for the bottle of the volume 0,75 lit with inner diameter of the neck 17,5-18,5 mm for keeping over 3 years. The orientational quantity 2.000.000 pcs. The length of the closure must be offered in the size 44,49 mm and 54 mm.

**The closures must meet European standards for the use in the food industry, with printed logo type of the buyer and must have the identification number.**

**SCREW CLOSURES FOR THE BOTTLE 1 LIT and 0,187 LIT**

* Screw closure with the plastic insertion with the ball for the bottle vol.1 Lit (colour and print according to the sample), measures 31,5 x 55 mm, orientiational quantity 350.000 pcs.
* Screw closure with saranex insertion for the bottle of 0,187 lit, measures 28,7 x 44 mm (colour and print according to the sample), orientational quantity 4.500.000 pcs.

**CROWN STOPPER**

 **•** Crown stopper with plastic insertion for the bottle of 1 lit, measures: inner diameter 26,6 +-

0,2 mm, outer diameter 32,1 +- 0,2 and height 6,75 +- 0,1 mm, orientational quantity

 5.300.000 pcs.

**PVC CAPS**

* PVC caps for the bottle 0,75 lit and 1 lit bottle without trigger, without print, measures 31 x 55 mm (colour according to the sample), package in the lines for machine setting, orientational quantity 9.000.000 pcs.
* PVC caps for the bottle 0,75 lit and 1 lit without trigger,with print,measures 31 x 55 mm (colour and print according to the sample), package in the lines for machine setting, orientational quantity 1.500.000 pcs.
* Caps for the sparkling wines (colour according to the sample), measures 34 x 120 mm, orientational quantity 60.000-70.000 pcs.
* Caps for the sparkling wines (colour according to the sample), measures 34 x 95 mm, orientational quantity 40.000 pcs.
* **Note:**

**The products must comply with the Food Industry Safety Standards and HACCP standards.Each delivery must be checked up at the receipt control in accordance with the prescribed documentation pursuant to ISO 9001: 2000.**

The Request comprises the annual needs by successive deliveries.

The Supplier is obliged that the subject of the delivery must completely comply with the contents of the request.

The offer should contain the following:

 -the title and main office of the company

-Decision of the company registration

-Decisions on Tax Identification No and VAT

-Card of the deposited signatures

-Confirmation by the competent court that the bankruptcy, liquidation and criminal proceedings has not been brought before the court

-Confirmation by the Tax Administration- Central registry of the economic entities that the company is not listed in the penalty register of the economic entities of the Tax administration

-Reference list

- Audited profit and loss account, balance sheet and balance of cash flows for the previous three years

-Time limit and parity of the delivery

-Prices per piece, without VAT

-Manner and conditions of payment

-Period of the guarantee of price

-Quality of the material

-Quality of the print

-Stability of the colours

-Reference list

- Option of the offer

Note: The requested quantities are not precise, because some deviations are possible regarding

 bigger or smaller quantities.

 The offers which are not complete and not sent in due time, shall not be taken into

 consideration.

 Foreign suppliers should send the documents which are in accordance with the regulations

 of the state, where they have a registered seat.

 The preparation and the other actions concerning the trial samples shall be at the expense of the Supplier.

Producers who cannot meet the whole quantity stated in the request,can apply to the Request, stating the quantities and conditions they can offer.

It is requested that the delivered closures comply with HACCP standards and have needed documentation, and each delivery shall be the subject of receipt control in accordance with the requests of ISO 9001 standard.

The offer for the transport package (wooden pallets and plastic supports), in case that the package is not returnable, may be sent.

The offers should be submitted in the closed envelope with the designation

-OFFER FOR closures and PVC caps - to the address:

 - 13.jul PLANTAZE- ad

Put Radomira Ivanovica 2

20 000 Podgorica

Montenegro

in the period from the 3rd of June 2015 to 30th of June 2015.

For further information,please call the Commercial Sector-Purchase Dept, every working day from 07-15 h, on the phone: +382-20-444-124Contact: Nenad Dulovic and in the Quality Dept. tel: +382 20 658 051 contact: Vukoman Vukovic.